MAKİNE BİLGİLERİ
==================================================

Makine Adı    : Jigger Thies
Marka         : Thies
Model         : 
Yıl           : 2015
Makine No     : MCH-000145
Durum         : 

--------------------------------------------------
AÇIKLAMA
--------------------------------------------------

The Thies NT Type jigger is engineered for dyeing a range of synthetic and blended fabrics&mdash;especially wide-open, crease-prone materials&mdash;at atmospheric (normal) temperatures (up to around 98 &deg;C) without applying pressure. Key features include: &bull; Full stainless steel construction: Durable and corrosion-resistant. &bull; A-frame drive (frequency-controlled) for fabric loading and unloading at preset winding tension. &bull; Fabric length controller that calculates and maintains both speed and tension throughout the process &bull; Weft device that allows lateral coiling of fabric during loading to ensure even distribution. &bull; High-efficiency variable-frequency motors that directly drive both main rollers for smooth, precise motion. &bull; Efficient dye tank design, delivering uniform results at low liquor ratios (economical dye usage) . &bull; Advanced automatic control using industrial PCs, PLCs, and fabric monitoring systems to maintain optimal parameters and flexibility for modern fiber blends. The Thies NT Type jigger (2300/2800) is a top-tier, atmospheric-temperature, wide-fabric dyeing machine that brings flexibility, precision, and cost-efficiency to textile finishing: &bull; Max Fabric Width: Up to 2850 mm (model 2300), up to 4100 mm (model 2800). &bull; Controls: Precise speed and tension control via modern automation systems (PLC, fabric monitoring). &bull; Build: Robust stainless steel, ensuring durability. &bull; Performance: Uniform results with low dye usage and excellent fabric quality (creaseless, evenly dyed). Year of construction: 2015 &bull; roller width: 3.000 mm &bull; fabric width: 2.800 mm &bull; fabric length, max. (with a fabric thickness &gt;= 0,3mm): 3.177m