MAKİNE BİLGİLERİ
==================================================

Makine Adı    : KUESTERS second hand bleaching line
Marka         : KUESTERS
Model         : 661
Yıl           : 1991
Makine No     : MCH-000211
Durum         : 

--------------------------------------------------
AÇIKLAMA
--------------------------------------------------

KUESTERS second hand bleaching line, 7 tanks with steamer, useful working width 4000 mm and 3800 mm - Manufacturer: KUESTERS - Year of construction: 1991 - Roller width: entry 4.000 mm, delivery 3.800 mm. - Useful working width: entry 3.800 mm, delivery 3.600 mm. - Production speed: up to 120 m/min. - Entry fabric from big batch with E+L selvedge widener mod. KF 2020 L - No. 1 washing tank model Compacta-D with fabric content 30 mt., useful working width 3.800 mm. - No. 1 squeezer mangle with two cylinders, type 225.23, useful working width 3.800 mm. - No. 1 washing tank model Maander with fabric content 15 m, useful working width 3.800 mm. - No. 1 cooling tank, useful working width 3.800 mm. - No. 1 high-performance two cylinders strong squeezer mangle with floating cylinder, type 222.56, useful working width 3.600 mm. - No. 1 impregnation tank to saturate the fabric, useful working width 3.600 mm. - No. 1 squeezer mangle with two cylinders, type 225.23, useful working width 3.600 mm. - No. 1 roller-bed vaporizer type 242.52, useful width 3.600 mm., with the following fabric loading capacities: 84 linear meters of cylinder fabric threading and 1.900 linear meters of fabric on the roller-bed. Date calculated with 150 gr./m2 fabrics. - No. 1 washing tank type 235.29 applied to the vaporizer, useful width 3.600 mm. - No. 1 squeezer mangle with two cylinders, type 225.23, useful working width 3.600 mm. - No. 1 washing tank model Compacta-D, useful working width 3.600 mm., fabric content 20 mt. -No. 1 squeezer mangle with two cylinders, type 225.23, useful working width 3.600 mm. - No. 1 washing tank model Maander, useful working width 3.600 mm., fabric content 15 m. No. 1 squeezer mangle with two cylinders, type 225.23, useful working width 3.600 mm. - No. 1 washing tank model Maander, useful working width 3.600 mm. - No. 1 cooling tank, useful width 3.600 mm. - No. 1 high-performance two cylinders strong squeezer mangle with floating cylinder, type 222.56, useful working width 3.600 mm. - Fabric delivery in big roll with tangential winding - Electrical cabinet - updated control pulpit with new screens - No. 2 heat recovery units