MAKİNE BİLGİLERİ
==================================================

Makine Adı    : Artos Latex Line
Marka         : ARTOS
Model         : 2003-2024
Yıl           : 2003
Makine No     : MCH-000050
Durum         : Çok İyi

--------------------------------------------------
AÇIKLAMA
--------------------------------------------------

Artos Latex Line Year of construction : 2024 Serial n&deg; : Working width: 1 meter to 2.6 meters Maximum setting width: 2.75 meters Speed: 1.7 meters to 35 meters per minute 1. Unwinding cradle: moves up and down hydraulically, the cradle is not powered. 2. Feeder J-Box 1: speed = 2 meters to 125 meters per minute 3. Feeder tank: working height approximately 3 meters 4. Sewing machine DOHLE: Type: Variant L7, maximum width = approximately 6 meters 5. J-Box 1: maximum useful height = 4.5 meters Feeding speed: 60 meters per minute With input pulling unit with coated roller and pneumatic pressure roller L/R controlled Speed adjustment by pendulum roller Automatic stop when empty 6. Beater/brush: adjustable on/off percentage Including dust extraction 7. Dust extraction system consisting of 2 parts: 1st part with a motor of 11 kW and 6 collection bags 2nd part with a motor of 15 kW and 6 collection bags Both are separately adjustable in speed 8. Turn frame control: 3-roller turn frame with motorized movement 9. Shearing machine 1: maximum height = 35 mm Unconnected dust extraction Wilhelm Kr&ocirc;gel 10. Shearing machine 2: maximum height = 28 mm Connected dust extraction Henri Paulus Spare cylinder provided 11. J-Box 2: maximum height = 4.5 meters Feeding speed linked to line speed, correction up to +200% With input pulling unit with coated roller and pneumatic pressure roller 12. Dust extraction on the back side of the fabric, width adjustable 13. Pendulum roller with pneumatic control 14. Turn frame control: 3-roller turn frame with motorized movement, 1 roller coated 15. Diagonal adjuster: electrically adjustable, manually operated 16. Doctor blade system with 2 applicator rollers + 2 pressure rollers to regulate tension, doctor blade Applicator roller diameter 400 mm, chrome-plated with drive, rotatable in both directions Correction up to 225% relative to line speed Applicator roller diameter 150 mm, chrome-plated with drive, rotatable in both directions Correction up to 175% relative to line speed Including automatic side control Motorized product distributor Applicator tray with a central recess to collect dirt Level measurement of the applicator tray 17. Foam table with adjustable gap opening, also tension control Can also be used as an air doctor blade!!! Including automatic side control Electric height adjustment, separately adjustable left and right Motorized product distributor Latex level measurement present 18. IR on gas divided over 2 fields part 1: 4 rows part 2: 3 rows Adjustable width from 1.5 meters to 2.5 meters 19. Automatic width adjuster (in service with TPE function) 20. TPE rollers (1 smooth roller &amp; 1 patterned roller) Gap opening between the 2 rollers is motorized adjustable Both rollers are equipped with cooling 21. Extruder movable on rails including dryer with approximately 750 kg capacity Maximum extruder speed = 400 rpm Maximum extruder output = approximately 750 kg/h Including additive addition 22. Cooler for patterned roller + extruder 23. Small compensator only used with TPE (buffer) Approximately 3 linear meters Height regulator present, linked to line speed 24. Foulard with 2 rollers (1 smooth &amp; 1 Bernie patterned) Pressure control with rollers Rollers are water-cooled Manually interchangeable Bottom roller is driven Correction possible relative to line speed 25. Oven: separated field (top and bottom) Top of the oven: 8 fields Bottom of the oven: 5 fields Ventilation adjustable per field Temperature settings depending on the type of yarn 26. Automatic CO₂ extinguishing system present (contains 29 bottles) 27. 2 compensators, each approximately 50 linear meters Motorized loading and unloading present Both compensators equipped with input pulling unit Input of compensator 1 equipped with a dancing roller with pressure regulator Stroke length approximately 800 mm Output of compensator 2 equipped with a dancing roller with pressure regulator Stroke length approximately 800 mm 28. Turn frame: 3 rollers with motorized movement, 1 roller coated 29. Longitudinal cutting installation 2 trimmers on the sides, manually operated Possibility of longitudinal cutting on both sides with a maximum of 5 longitudinal knives These are manually operated together 30. Rewinder: this is hydraulically tiltable Winding rollers diameter 320 mm L/R movement via spindle motor The winding tension is adjustable Length measurement provided 31. Discharge table consisting of 3 parts Part 1: length approximately 6 meters Part 2: length approximately 8 meters Part 3: length approximately 3 meters; this last part is tiltable 32. Latex kitchen consisting of 4 stainless steel tanks, each 1500 liters All equipped with an agitator On the ground floor, 2 filters with removable baskets (stainless steel) are provided 33. Mixer: Mixer Company, single head Liter weight adjustable from 150 g/l to 1250 g/l Mixer head speed: 50 rpm to 150 rpm Maximum flow rate = approximately 2000 kg/h 34. Pump PERISTALTIC PUMP HELIOS ASP 32 FX Max Flow rate: 2940 liters/hour - 70 rpm - 1.1 kW - 3-phase Hose: Natural Rubber