MAKİNE BİLGİLERİ
==================================================

Makine Adı    : Artos Latex Line
Marka         : ARTOS
Model         : 2003-2024
Yıl           : 2003
Makine No     : MCH-000050
Durum         : Çok İyi

--------------------------------------------------
AÇIKLAMA
--------------------------------------------------

Artos Latex Line
Year of construction : 2024
Serial n° :
Working width: 1 meter to 2.6 meters
Maximum setting width: 2.75 meters
Speed: 1.7 meters to 35 meters per minute
1.	Unwinding cradle: moves up and down hydraulically, the cradle is not powered.

2.	Feeder J-Box 1: speed = 2 meters to 125 meters per minute

3.	Feeder tank: working height approximately 3 meters

4.	Sewing machine DOHLE: Type: Variant L7, maximum width = approximately 6 meters

5.	J-Box 1: maximum useful height = 4.5 meters 
Feeding speed: 60 meters per minute 
With input pulling unit with coated roller and pneumatic pressure roller 
L/R controlled 
Speed adjustment by pendulum roller 
Automatic stop when empty

6.	Beater/brush: adjustable on/off percentage 
Including dust extraction

7.	Dust extraction system consisting of 2 parts: 
1st part with a motor of 11 kW and 6 collection bags 
2nd part with a motor of 15 kW and 6 collection bags 
Both are separately adjustable in speed

8.	Turn frame control: 3-roller turn frame with motorized movement

9.	Shearing machine 1: maximum height = 35 mm
Unconnected dust extraction Wilhelm Krôgel

10.	Shearing machine 2: maximum height = 28 mm 
Connected dust extraction Henri Paulus 
Spare cylinder provided

11.	J-Box 2: maximum height = 4.5 meters 
Feeding speed linked to line speed, correction up to +200% 
With input pulling unit with coated roller and pneumatic pressure roller

12.	Dust extraction on the back side of the fabric, width adjustable

13.	Pendulum roller with pneumatic control

14.	Turn frame control: 3-roller turn frame with motorized movement, 1 roller coated

15.	Diagonal adjuster: electrically adjustable, manually operated

16.	Doctor blade system with 2 applicator rollers + 2 pressure rollers to regulate tension, doctor blade
Applicator roller diameter 400 mm, chrome-plated with drive, rotatable in both directions
Correction up to 225% relative to line speed
Applicator roller diameter 150 mm, chrome-plated with drive, rotatable in both directions
Correction up to 175% relative to line speed
Including automatic side control
Motorized product distributor
Applicator tray with a central recess to collect dirt
Level measurement of the applicator tray

17.	Foam table with adjustable gap opening, also tension control
Can also be used as an air doctor blade!!!
Including automatic side control
Electric height adjustment, separately adjustable left and right
Motorized product distributor
Latex level measurement present

18.	IR on gas divided over 2 fields
part 1: 4 rows
part 2: 3 rows
Adjustable width from 1.5 meters to 2.5 meters

19.	Automatic width adjuster (in service with TPE function)

20.	TPE rollers (1 smooth roller & 1 patterned roller)
Gap opening between the 2 rollers is motorized adjustable
Both rollers are equipped with cooling

21.	Extruder movable on rails including dryer with approximately 750 kg capacity
Maximum extruder speed = 400 rpm
Maximum extruder output = approximately 750 kg/h
Including additive addition

22.	Cooler for patterned roller + extruder

23.	Small compensator only used with TPE (buffer)
Approximately 3 linear meters
Height regulator present, linked to line speed

24.	Foulard with 2 rollers (1 smooth & 1 Bernie patterned)
Pressure control with rollers
Rollers are water-cooled
Manually interchangeable
Bottom roller is driven
Correction possible relative to line speed
25.	Oven: separated field (top and bottom)
Top of the oven: 8 fields
Bottom of the oven: 5 fields
Ventilation adjustable per field
Temperature settings depending on the type of yarn

26.	Automatic CO₂ extinguishing system present (contains 29 bottles)

27.	2 compensators, each approximately 50 linear meters
Motorized loading and unloading present
Both compensators equipped with input pulling unit
Input of compensator 1 equipped with a dancing roller with pressure regulator
Stroke length approximately 800 mm
Output of compensator 2 equipped with a dancing roller with pressure regulator
Stroke length approximately 800 mm

28.	Turn frame: 3 rollers with motorized movement, 1 roller coated

29.	Longitudinal cutting installation
2 trimmers on the sides, manually operated
Possibility of longitudinal cutting on both sides with a maximum of 5 longitudinal knives
These are manually operated together

30.	Rewinder: this is hydraulically tiltable
Winding rollers diameter 320 mm
L/R movement via spindle motor
The winding tension is adjustable
Length measurement provided

31.	Discharge table consisting of 3 parts
Part 1: length approximately 6 meters
Part 2: length approximately 8 meters
Part 3: length approximately 3 meters; this last part is tiltable

32.	Latex kitchen consisting of 4 stainless steel tanks, each 1500 liters
All equipped with an agitator
On the ground floor, 2 filters with removable baskets (stainless steel) are provided

33.	Mixer: Mixer Company, single head
Liter weight adjustable from 150 g/l to 1250 g/l
Mixer head speed: 50 rpm to 150 rpm
Maximum flow rate = approximately 2000 kg/h

34.	Pump PERISTALTIC PUMP HELIOS ASP 32 FX
Max Flow rate: 2940 liters/hour - 70 rpm - 1.1 kW - 3-phase
Hose: Natural Rubber