MAKİNE BİLGİLERİ
==================================================

Makine Adı    : Calandru Ramisch
Marka         : Ramisch
Model         : NIPCO CALENDER
Makine No     : MCH-000139
Durum         : 

--------------------------------------------------
AÇIKLAMA
--------------------------------------------------

NIPCO CALENDER &ndash; WIDTH 3000 MM With Nipco L rollers by Voith paper Whether producing shirts, ladies fashion, underwear, bed sheets, table linen, home textiles or protective clothing, the system allows you to compete in the market. The hydrostatic support elements of NIPCO&trade; L system are independently arranged in a 90&deg; configuration, one active against a steel bowl, one active against a cotton bowl. The stabilising force angle of 270&deg; will at all times guarantee a free and uniform turn of the sleeve. With those independent pressure lines in action you may "play" with your pressure settings. High glazing: increased pressure in the nip Steel/NIPCO&trade;, same time slightly reduced glazing and softer handle, decreased pressure setting in the nip NIPCO&trade;/Cotton. Elegant glazing and remarkable softness in handle: decreased pressure in the nip Steel/NIPCO&trade;, same time increased pressure in the nip NIPCO&trade;/Cotton. &bull; Ramisch Guarneri &bull; Nipco L Calander type RGK.390.3000 &bull; manufacturer: Ramisch Guarneri &bull; Year of construction: 2013 &bull; fabric entry: from big roll &bull; Roller surface width: 3.000mm &bull; Max. fabric width: 2.800mm &bull; Min. fabric width: 1.000mm &bull; Roller arrangement : Steel top roller diameter: approx 440mm &bull; NipcoL bottom roller diameter: approx 500mm &bull; Cotton back roller diameter: approx. 750mm &bull; Heating system: Electro/ hot water &bull; Speed from 5 to 80m/min &bull; Hydraulic working pressure 50 to 300 N/mm &bull; Steel roller temperature up to 210 Celsius &bull; fabric delivery: in big roll &bull; purpose of machine: rolling, glazing, chintz softness and smoothing effects