MAKİNE BİLGİLERİ
==================================================

Makine Adı    : SALVADE continuous steam flash ager steamer after printing
Marka         : SALVADE
Model         : 
Yıl           : 2018
Makine No     : MCH-000181
Durum         : 

--------------------------------------------------
AÇIKLAMA
--------------------------------------------------

SALVADE continuous steam flash ager steamer after printing year 2018, fabric content 180 mt, roller width 2300 mm - Brand: SALVADE - Model: VPM - Year of construction: 2018 - Roller width: 2.300 mm - Working width: 2.000 mm - Fabric content inside machine: 180 mt - Fans for steam recycling - Rotating inlet spreader with bypass system and Teflon-coated cylinders - conveyor belt for introducing elastic fabrics (Mesh and Shuttle) with end-of-fabric photocell - Protection paper winding unit with constant pull control - Predisposition for high temperature operation - Adjustment of rotation speed of fabric holder rods - Automatic chain lubrication - Teleservice - Fan adjustment by inverter - SuperWet Temperature control and steam saturation system - Walkable grille 180 m - End-of-fabric photocell - One hot Teflon-coated and controlled cylinder diam. 220 mm w.w. 2000 mm - Controlled roller entry for elastic and delicate fabrics - Automatic humidification system - Steam consumption control - Automatic steam regulation valves - Entrance and exit same side with conveyor belt - Steam distributor in iron DN65 (Clarino) - Machine suitable for woven and knitting fabrics